[Contents] [Prev] [Next] [Report an Error]

# OC12/STM4 ATM Multimode With APS/MSP Redundancy Module Combination

> Line module label | OCx/STMx ATM or OCx/STMx /DS3-ATM
> I/O module label | OC12 STM4 APS MULTI MODE
> Number of I/O ports | 1 active, 1 redundant
> Software release | First supported: 2.0.0 (128 MB), 5.0.0 (256 MB) Final supported: Not applicable The OCx/STMx ATM line module or the OCx/STMx /DS3-ATM line module must have a minimum of 256 MB of memory to be used with JUNOSe Release 5.3.0 or a higher-numbered release.
> Description | 130 W Can use either the 128-MB OCx/STMx ATM line module or the 256-MB OCx/STMx /DS3-ATM line module. Unchannelized, concatenated OC12/STM4 for ATM
> Type | EFA ASIC
> Capability | OC12/STM4 ATM/AAL5
> Software features | See OCx/STMx ATM Modules for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX-7xx models ERX-14xx models ERX-310 router
> SRP module compatibility | SRP-5G+ SRP-10G SRP-40G SRP-40G PLUS SRP-SE10G
> Module redundancy support | 1:N redundancy NOTE: Line module redundancy is not supported on the ERX-310 router.
> Cables and connectors | SC full duplex Tx power: min: –19 dBm max: –14 dBm Center wavelength: 1310 nm Rx input power: min: –30 dBm max: –14 dBm Rated for 2 km (1.2 miles) over 62.5-micron core cable with an optical loss of 0–9 dB or 50-micron core cable with an optical loss of 7 dB See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See Module LEDs.
> Alarms, errors, and events | See Monitoring SONET/SDH Interfaces in JUNOSe Physical Layer Configuration Guide, Chapter 3, Configuring Unchannelized OCx/STMx Interfaces.

[Contents] [Prev] [Next] [Report an Error]