[Contents] [Prev] [Next] [Index] [Report an Error]

# write memory

#### Syntax

write memory

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Saves all outstanding (unsaved) configuration changes to nonvolatile storage; an exact alias of the copy running-configuration startup-configuration command. Available if the router is in either Automatic Commit mode or Manual Commit mode. If issued while in Automatic Commit mode, the CLI notifies you that the command is not necessary, but allows you to proceed. There is no no version.

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]