[Contents] [Prev] [Next] [Index] [Report an Error]

# link failover timeout

#### Syntax

link failover timeout failTime

no link failover timeout

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the time that the router waits for a port on a GE I/O module to become active before the router switches to the redundant port. The no version restores the default setting, in which the router sets this time automatically.

#### Options

- failTime—Time that the router waits; in the range 100–10000 ms

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]