[Contents] [Prev] [Next] [Index] [Report an Error]

# atm auto-configuration

#### Syntax

[ no ] atm auto-configuration

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables autoconfiguration of ILMI. Autoconfiguration is enabled by default. This command overrides any previous configuration of the atm uni-version command. The no version disables auto configuration and sets the ILMI parameters to the UNI version configured using the atm uni-version command, which has a default value of UNI 4.0.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]