[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 mld ssm-map static

#### Syntax

[ no ] ipv6 mld ssm-map static accessListName sourceAddress

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies an access list and source address for use in SSM mapping. SSM mapping statically assigns sources to MLDv1 groups. You must use SSM mapping for MLDv1 hosts to interoperate with PIM SSM. SSM mapping allows the router to use a statically configured list to translate <*,G> memberships to <S,G> memberships. The no version removes the SSM map association.

| Note: To operate correctly, the static source addresses configured with the ipv6 mld ssm-map static command must fall within the configured PIM SSM range.

#### Options

- accessListName—Name of the access control list
- sourceAddress—Address of the source

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]