[Contents] [Prev] [Next] [Index] [Report an Error]

# frequency

#### Syntax

frequency frequencyValue

no frequency

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

In RTR Configuration mode, sets the time interval between RTR operations. In SNMP Event Manager Configuration mode, sets the frequency (in seconds) at which you want MIB sampling to occur. The no version restores the default value.

#### Options

- frequencyValue—Number of seconds between RTR operations or MIB sampling operations, depending on the configuration mode; with RTR operations, for both types (echo and pathEcho), the default value is 60 seconds; with MIB sampling, the default value is 600 seconds.

#### Mode

RTR Configuration, SNMP Event Manager Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]