[Contents] [Prev] [Next] [Index] [Report an Error]

# radius authentication server

#### Syntax

[ no ] radius authentication server ipAddress

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the IP address of a RADIUS authentication server and puts the E-series router into RADIUS Configuration mode. The no version deletes the instance of the RADIUS server.

#### Options

- ipAddress—IP address of the server

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]