[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring AAA Profile Configuration

#### Purpose

Display the configuration of all AAA profiles or of a specific profile.

#### Action

To display the configuration of all AAA profiles or of a specific profile:

    host1#show aaa profile name PreAuth1
    preAuth1:
        atm nas-port-type: ADLSL-CAP
        ethernet nas-port-type: Cable
        profile-service-description: xyzService
        pre-authenticate
        allow xyz.com
        deny default
        translate xyz1.com abc.com

#### Meaning

Table 13 Lists the show aaa profile command output fields.

Table 13: show aaa profile Output Fields

Field Name | Field Description
--- | ---
atm nas-port-type | Configuration of NAS-Port-Type attribute for ATM interfaces
ethernet nas-port-type | Configuration of NAS-Port-Type attribute for Ethernet interfaces
profile-service-description | Description configured in the Service-Description attribute
pre-authenticate | Indicates that subscriber preauthentication is configured for the profile
allow | One or more domain names that are allowed access to AAA authentication
deny | One or more domain names that are denied access to AAA authentication
translate | Original domain name and the name to which it is mapped for domain map lookup

#### Related Topics

- show aaa profile

[Contents] [Prev] [Next] [Index] [Report an Error]