[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 mld robustness

#### Syntax

ipv6 mld robustness numberOfMessages

no ipv6 mld robustness

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the number of times that the router sends MLD group-specific queries before declaring a group to no longer have any members on an interface. The no version restores the default value, 2.

#### Options

- numberOfMessages—Number of times that the router sends MLD group-specific queries in the range 1–4

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]