[Contents] [Prev] [Next] [Index] [Report an Error]

## ha

#### Description

High availability messages

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Accessing redundancy mode is not supported on the standby SRP; changing redundancy mode is not supported on the standby SRP; high availability disabled due to state error

#### Warning Log

High availability disabled due to incompatible release on standby; high availability disabled due to user initiated disable

#### Notice Log

High availability disabled due to standby down; high availability is now active

#### Info

None

#### Debug

None

#### Filter

None

[Contents] [Prev] [Next] [Index] [Report an Error]