[Contents] [Prev] [Next] [Index] [Report an Error]

# bgp wait-on-end-of-rib

#### Syntax

bgp wait-on-end-of-rib seconds

no bgp wait-on-end-of-rib

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Specifies how long BGP waits to receive an End-of-RIB marker sent by route-target address family peers to signal the peer has finished advertising route-target membership information. Applies to all peers in the route-target address family. The no version restores the default value.

#### Options

- seconds—Number of seconds BGP wait for End-of-RIB marker, in the range 1–3600; default is 60 seconds

#### Mode

Address Family Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]