[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring MPLS Minor Interfaces

Purpose

Display status and configuration information about MPLS minor interfaces.

The show mpls interface minor command displays the same information.

Action

To display information about MPLS minor interfaces:

    host1:pe1#show mpls minor-interface
    MPLS minor interface pe1-to-pe2 (transmit)
      Stacked on MPLS major ATM2/0.10
      Operational state is up
      Sent:
        0 packets
        0 bytes

      queue 0: traffic class best-effort, bound to atm-vc ATM2/0.10
        Queue length 0 bytes
        Forwarded packets 0, bytes 0
        Dropped committed packets 0, bytes 0
        Dropped conformed packets 0, bytes 0
        Dropped exceeded packets 0, bytes 0

    MPLS minor interface lsp-02020202-1-4 (receive)
      Stacked on MPLS major ATM2/0.10
      Operational state is up
      Statistics not enabled for this interface

To display detailed information about MPLS minor interfaces:

    host1:pe1#show mpls minor-interface detail
    MPLS minor interface pe1-to-pe2 (transmit)
      Stacked on MPLS major ATM2/0.10
      Operational state is up
      MPLS minor interface UID is 0x1a000001
      Lower MPLS major interface UID is 0x19000001
      Sent:
        0 packets
        0 bytes

      queue 0: traffic class best-effort, bound to atm-vc ATM2/0.10
        Queue length 0 bytes
        Forwarded packets 0, bytes 0
        Dropped committed packets 0, bytes 0
        Dropped conformed packets 0, bytes 0
        Dropped exceeded packets 0, bytes 0

    MPLS minor interface lsp-02020202-1-4 (receive)
      Stacked on MPLS major ATM2/0.10
      Operational state is up
      MPLS minor interface UID is 0x1a000004
      Lower MPLS major interface UID is 0x19000001
      Statistics not enabled for this interface

To display summary information about MPLS minor interfaces:

    host1:pe1#show mpls minor-interface brief
                         Lower     Oper
       Interface       MplsMajor   state   Direction
    ----------------   ---------   -----   ---------
    pe1-to-pe2         ATM2/0.10   up      transmit
    lsp-02020202-1-4   ATM2/0.10   up      receive
    ERX-01-0c-d7:pe1#

Meaning

Table 47 lists the show mpls minor-interface command output fields.

Table 47: show mpls minor-interface Output Fields

Field Name | Field Description
--- | ---
Interface | Specifier and status of each interface

#### Related Topics

- show mpls minor-interface

[Contents] [Prev] [Next] [Index] [Report an Error]