[Contents] [Prev] [Next] [Index] [Report an Error]

# ip rsvp authentication

#### Syntax

[ no ] { ip | mpls } rsvp authentication

#### Description

Enables MD5 authentication on the RSVP interface in implementations on routers from other vendors. See the mpls rsvp authentication command for a complete description and syntax.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]