[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the DSL-Port-Type RADIUS Attribute

#### Purpose

Display the DSL port type for NAS-Port-Type attribute for ATM and Ethernet users.

#### Action

To display the DSL port type for NAS-Port-Type attribute for ATM users:

    host1#show radius dsl-port-type
    xdsl

To display the NAS-Port-Type attribute for Ethernet interfaces:

    host1#show radius ethernet-port-type
    virtual

#### Related Topics

- show radius dsl-port-type
- show radius ethernet-port-type

[Contents] [Prev] [Next] [Index] [Report an Error]