[Contents] [Prev] [Next] [Index] [Report an Error]

# tcp resequence-buffers default-vr-maximum

#### Syntax

[ ip ] tcp resequence-buffers default-vr-maximum defaultVrMaxValue

no [ ip ] tcp resequence-buffers default-vr-maximum

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
ip keyword made optional in JUNOSe Release 7.2.0.

#### Description

Specifies the default buffer limit assigned to all virtual routers when the virtual router is established. Specifying a value of zero (0) turns off the limit assignment. The no version reverts the virtual router maximum value to its default (100 buffers).

#### Options

- ip—Optional keyword for use with older scripts
- defaultVrMaxValue—Default number of maximum buffers for newly established virtual routers, in the range 1–65535

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]