[Contents] [Prev] [Next] [Index] [Report an Error]

# distance ip

#### Syntax

[ no ] distance weight ip

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the administrative distance for IS-IS routes that are inserted into the IP routing table. A distance of 255 prevents the route from being installed in the routing table. The no version restores the default value, 115.

#### Options

- weight—Administrative distance assigned to IS-IS routes added to the IP routing table in the range 1–255

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]