[Contents] [Prev] [Next] [Index] [Report an Error]

# encapsulation frame-relay ietf

#### Syntax

encapsulation frame-relay ietf

no encapsulation frame-relay

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables Frame Relay encapsulation. The no version removes Frame Relay configuration from an interface.

#### Mode

Interface Configuration

#### Related Topics

- Configuring Frame Relay Layer 2 Services in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]