[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the QoS Configuration of ATM Interfaces

#### Purpose

Display ATM port queuing mode and QoS shaping mode status for a specific ATM interface.

#### Action

To display the QoS configuration on an ATM interface:

    host1# show interfaces atm 2/0
    ATM Interface 2/0 is up, line protocol is disabled
    AAL5 operational status:       up
          time since last status change: 01:08:32
    ATM operational status:        up
          time since last status change: 01:08:32
    .
    .
    .....
    InPackets:        0
    InBytes:          0
    InCells:          0
    OutPackets:       7803262
    OutBytes:         7803262000
    OutCells:         163868502
    InErrors:         0
    OutErrors:        0
    InPacketDiscards: 0
    InByteDiscards:   0
    InCellErrors:     0
    Administrative qos-shaping-mode: frame
    Operational qos-shaping-mode: frame
    Administrative qos-mode-port: none
    Operational qos-mode-port: none
    Attached QoS profile: shaping

#### Meaning

Table 49 lists the related show interfaces atm command output fields.

Table 49: show interfaces atm Output Fields

Field Name | Field Description
--- | ---
Administrative qos-mode-port | Per-port queuing mode status: disabled, low-latency, low-cdv, none
Operational qos-mode-port | Per-port queuing mode status: disabled, low-latency, low-cdv, none
Administrative qos-shaping-mode | QoS shaping mode: disabled frame cell none
Operational qos-shaping-mode | QoS shaping mode: disabled frame cell none
Attached QoS profile | QoS profile attachment at or below the displayed interface. For example, if the interface being displayed is a VC, and the attachment is at the ATM AAL5 interface, the ATM AAL5 interface attachment is displayed.

#### Related Topics

- Configuring the QoS Shaping Mode for ATM Interfaces
- Configuring a QoS Profile
- Attaching a QoS Profile to an Interface
- Creating Parameter Instances
- For more information about other fields displayed with this command, see JUNOSe Link Layer Configuration Guide
- show atm interface command
- show interfaces atm command

[Contents] [Prev] [Next] [Index] [Report an Error]