[Contents] [Prev] [Next] [Index] [Report an Error]

# path snmp trap link-status

#### Syntax

For channelized OCx/STMx interfaces:

[ no ] path pathChannel snmp trap link-status

For unchannelized OCx/STMx interfaces:

[ no ] path snmp trap link-status

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables SNMP link-status processing for the path layer of SONET and SDH interfaces. The no version disables SNMP link-status processing.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path on a channelized interface

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]