[Contents] [Prev] [Next] [Index] [Report an Error]

# atm-vp qos-profile

#### Syntax

[ no ] atm-vp vpi qos-profile qosProfileName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Attaches a QoS profile to the specified VP on the interface. The no version detaches the QoS profile from the VP.

#### Options

- vpi—Virtual path identifier of this PVC; number in the range 0–255
- qosProfileName—Name of the QoS profile that you want to attach to the VP

#### Mode

Interface Configuration

#### Related Topics

- Attaching a QoS Profile to an Interface

[Contents] [Prev] [Next] [Index] [Report an Error]