[Contents] [Prev] [Next] [Index] [Report an Error]

# key-string

#### Syntax

key-string keyStringData

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Manually configures a 1024-bit or 2048-bit ISAKMP/IKE public key that a remote peer uses for RSA authentication without the need for a digital certificate. The key string represents the public key hexadecimal data that includes the ASN.1 object identifier and sequence tags for RSA encryption. There is no no version. To remove a peer public key from the router, use the no version of the ipsec key pubkey-chain rsa command.

#### Options

- keyStringData—Alphanumeric string with a maximum length of 1999 characters; delimited by the first character of the string, which must be repeated at the end of the string and must not occur anywhere else in the string

#### Mode

IPSec Peer Public Key Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]