[Contents] [Prev] [Next] [Index] [Report an Error]

# atm

#### Syntax

atm { ubr | ubrpcr pcr | nrtvbr pcr scr mbs | rtvbr pcr scr mbs | cbr pcr }

no atm

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures traffic-shaping parameters for PPPoA via domain-based parameters. The no version removes the ATM traffic-shaping configuration.

#### Options

- ubr—Sets the traffic category to unspecified bit rate
- ubrpcr—Sets the traffic category to unspecified bit rate with peak cell rate
- nrtvbr—Sets the traffic category to non–real time variable bit rate
- rtvbr—Set the traffic category to real time variable bit rate
- cbr—Sets the traffic category to constant bit rate
- pcr—Peak cell rate in the range 0–4294967295 Kbps
- scr—Sustained cell rate in the range 0–4294967295 Kbps
- mbs—Maximum burst size in the range 0–4294967295 Kbps

#### Mode

Domain Map Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]