[Contents] [Prev] [Next] [Index] [Report an Error]

## connectionManager

#### Description

Logging various conditions in the component that manages the chassis fabric.

#### Emergency

None

#### Alert

None

#### Critical

10G and 5G SRP modules only—Detection that the FPGAs have not been loaded (results in an SRP [and chassis] reset)

#### Error

10G and 5G SRP modules only—That there is not enough bandwidth for a particular board in the system, that connections could not be added in the fabric due to resource limitations (such as memory), that a board was just removed and the resource will not be needed when this condition is detected momentarily, or that a connection cannot be closed or a multicast destination cannot be dropped.

#### Warning Log

Cannot connect to a particular source or destination address (board may have just been removed)

#### Notice Log

A connection that previously could not be closed has now closed; a multicast destination that previously could not be dropped has now been dropped

#### Info

Various logs to indicate events and transitions for low level diagnosis

#### Debug

Various logs to indicate events and transitions for low level diagnosis

#### Filter

None

[Contents] [Prev] [Next] [Index] [Report an Error]