[Contents] [Prev] [Next] [Index] [Report an Error]

# clear arp

#### Syntax

clear [ ip ] arp [ vrf vrfName ] { ipAddress interfaceType interfaceSpecifier | * }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Clears entries from the ARP cache. There is no no version.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- ipAddress—IP address in 32-bit dotted-decimal format of the entry to be cleared
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- *—Clears all dynamic ARP entries

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]