[Contents] [Prev] [Next] [Index] [Report an Error]

# radius remote-circuit-id-delimiter

#### Syntax

radius remote-circuit-id-delimiter delimiter

no radius remote-circuit-id-delimiter

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the delimiter character that sets off components in the PPPoE remote circuit ID value sent from a DSLAM and captured on the router. The no version restores the default delimiter character, #.

#### Options

- delimiter—Special character (for example, ! or %) to set off components in the PPPoE remote circuit ID value captured from a DSLAM; the default delimiter character is #

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]