[Contents] [Prev] [Next] [Index] [Report an Error]

# snmp-server host

#### Syntax

To specify the SNMP version, community, UDP port, trap category and trap severity:

snmp-server host ipAddress [ version ver ] securityString [ udp-port port ]
[ trapCategory ]* [ trapFilters trapFilter ]

no snmp-server host ipAddress

To specify the ping timeout and trap queue:

snmp-server host ipAddress pingTimeOut timeOutValue
[ trapQueue { drainRate queueDrainRate | full queueFull |
size queueSize }
[ drainRate queueDrainRate | full queueFull | size queueSize ]*]

snmp-server host ipAddress trapQueue
{ drainRate queueDrainRate | full queueFull | size queueSize }
[ drainRate queueDrainRate | full queueFull | size queueSize ]*
[ pingTimeOut timeOutValue ]

no snmp-server host ipAddress { pingTimeOut | trapQueue { drainRate | full | size } }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
ip keyword added in JUNOSe Release 7.1.0.
packetMirror keyword added in JUNOSe Release 7.2.0.

#### Description

Configures one or more hosts to receive an SNMP trap. The no version removes the specified host from the list of recipients.

#### Options

- ipAddress—IP address of the SNMP trap recipient
- ver—SNMP protocol version for traps sent to host; one of the following values: v1, v2c, or v3
- securityString—SNMP community string
- port—UDP port number of SNMP trap recipient
- trapCategory—SNMP trap category
  - addrPool—Local address pool traps
  - atmPing—E-series router proprietary ATM ping traps
  - bfdmib—BFD MIB traps
  - bgp—BGP state change traps
  - bulkstats—Bulkstats file full and nearly full traps
  - cliSecurityAlert—Security alerts traps
  - dosProtectionPlatform—DoS protection platform traps
  - dvmrp—DVMRP traps
  - dvmrpUni—E-series router proprietary DVMRP traps
  - environment—Power/temperature/fan traps
  - fileXfer—File transfer status change traps
  - inventory—Router inventory/status traps
  - ip—Internet Protocol traps
  - ldp—LDP traps
  - link—SNMP linkUp/linkDown traps
  - log—System log capacity traps
  - mobileIpv4—Mobile IPv4 traps
  - mplste—Mplste traps
  - mrouter—Mrouter traps
  - packetMirror—Secure packet mirroring traps; visible only if packet mirroring is enabled
  - ospf—OSPF traps
  - ping—Ping operation traps (in disman remops MIB)
  - radius—RADIUS traps
  - snmp—SNMP coldstart, warmstart, link, authenticationFailure traps
  - traceroute—Traceroute operation traps (in disman remops MIB)
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- trapFilter—Minimum severity level for filtering traps sent to this host
  - alert—Severity level 1
  - critical—Severity level 2
  - debug—Severity level 7
  - emergency—Severity level 0
  - error—Severity level 3
  - informational—Severity level 6
  - notice—Severity level 5
  - warning—Severity level 4
- timeOutValue—Ping timeout in minutes, in the range 1–90; default value is 1
- trapQueue—Configures the SNMP trap queue for traps sent to this host
- queueDrainRate—Maximum number of traps per second to be sent to the host, in the range 0–2147483647; default value is 0
- queueFull—Method used to drop traps when the trap queue is full
  - dropFirstIn—Drops the oldest trap in the queue
  - dropLastIn—Drops the most recent trap added to the queue
- queueSize—Maximum number of traps to be kept in the trap queue, in the range 32–214748364; default value is 32

#### Mode

Global Configuration

#### Related Topics

- Monitoring SNMP Secure Packet Mirroring Traps

[Contents] [Prev] [Next] [Index] [Report an Error]