[Contents] [Prev] [Next] [Index] [Report an Error]

# ip pim join-prune-interval

#### Syntax

ip pim join-prune-interval interval

no ip pim join-prune-interval

#### Release Information

Command introduced in JUNOSe Release 10.0.0.

#### Description

Specifies the time interval at which the router sends the PIM join/prune message to the upstream RPF neighbor. In Interface Configuration mode, the no version restores the value that is specified in Router Configuration mode. If the message interval is not specified in Router Configuration mode, then the default value of 60 seconds is restored.

| Note: You cannot configure the designated router priority on PIM dense mode interfaces.

#### Options

- interval—Interval in the range 10–210 seconds at which the router sends the PIM join/prune message; the default value is 60 seconds.

#### Mode

Interface Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]