[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring SNMP Secure Packet Mirroring Traps

#### Purpose

Display configuration information about SNMP traps and trap destinations. The PacketMirror trap category is displayed only when the mirror enable command has been configured. The Secure Trap Logging status is displayed only when the mirror enable command has been issued and secure audit logs have been configured.Text in bold indicates secure packet mirroring trap configuration information.

#### Action

To display secure packet mirroring traps:

    host1# show snmp trap
    Enabled Categories: CliSecurity,  PacketMirror , Sonet
    SNMP authentication failure trap is disabled
    Trap Source: FastEthernet 6/0, Trap Source Address:192.168.120.78
    Trap Proxy: enabled
    Secure Trap Logging is enabled
    Global Trap Severity Level: 6 - informational
    Address          Security String                   Ver  Port   Trap Categories
    ---------------  --------------------------------  ---  -----  ----------------
    10.1.1.1         host1                             v1     162  Cli
    10.12.12.12      secureHost                        v3     162  CliOspf PacketMirror Sonet
    192.168.57.162   host2                             v3     162  Sonet
    Address         TrapSeverityFilter  Ping    Maximum    Queue    Queue Full
                                       TimeOut QueueSize DrainRate discrd methd
    --------------- ------------------ ------- --------- --------- -------------
    10.1.1.1        5 - notice         1       32        0         dropLastIn
    10.12.12.12     2 - critical       1       32        0         dropLastIn
    192.168.57.162  2 - critical       1       32        0         dropLastIn

#### Meaning

Table 64 lists the show snmp trap command output fields.

Table 64: show snmp trap Output Fields

Field Name | Field Description
--- | ---
Enabled Categories | Trap categories that are enabled on the router
SNMP authentication failure trap | Enabled or disabled
Trap Source | Interface whose IP address is used as the source address for all SNMP traps
Trap Source Address | IP address used as the source address for all SNMP traps
Trap Proxy | Enabled or disabled
Secure Trap Logging | Enabled or disabled
Global Trap Severity Level | Global severity level filter; if a trap does not meet this severity level, it is discarded
Address | IP address of the trap recipient
Security String | Name of the SNMP community
Ver | SNMP version (v1 or v2) of the SNMP trap packet
Port | UDP port on which the trap recipient accepts traps
Trap Categories | Types of traps that the trap recipient can receive
TrapSeverityFilter | Severity level filter for this SNMP host
Ping TimeOut | Configured ping timeout in minutes
Maximum QueueSize | Maximum number of traps to be kept in the trap queue
Queue DrainRate | Maximum number of traps per second to be sent to the host
Queue Full discrd methd | Method used to discard traps when the queue is full:
dropFirstIn | Oldest trap in the queue is dropped
dropLastIn | Most recent trap is dropped

#### Related Topics

- mirror trap-enable
- snmp-server enable traps
- snmp-server host
- snmp-server secure-log
- show mirror trap
- show snmp trap

  | Note: Secure packet-mirroring trap configuration information appears in the Enabled Categories and Trap Categories fields only if the mirror-enable command is enabled.

[Contents] [Prev] [Next] [Index] [Report an Error]