[Contents] [Prev] [Next] [Index] [Report an Error]

# multicast group port limit

#### Syntax

multicast group port interfaceSpecifier limit groupLimit

no multicast group port interfaceSpecifier limit

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Limits the number of IGMP or MLD groups that a port can accept. The no version restores the default situation, in which there is no limit to the number of IGMP or MLD groups the port can accept.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- groupLimit—Maximum number of IGMP or MLD groups that an interface can accept in the range 0–64,000

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]