[Contents] [Prev] [Next] [Index] [Report an Error]

# table-map

#### Syntax

table-map mapTag

For removing route maps for IS-IS IPv6 only:

no table-map

For removing route maps for all other cases:

no table-map [ mapTag ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Applies the specified route map to all BGP, IS-IS, OSPF, or RIP routes about to be added to the IP routing table. The no version halts application of the route map.

#### Options

- mapTag—A string of up to 32 alphanumeric characters that specifies the name of the route map; for each protocol, the route map can set only the following values:
  - BGP—Distance, IP next hop, level, metric, metric type, route type, and tag values
  - IS-IS—Distance, level, metric, metric type, origin, preference, route type, and tag values; IS-IS IPv6 supports only a single route map
  - OSPF—Distance, metric, metric type, route type, and tag values
  - RIP—Distance, metric, and tag values

#### Mode

Address Family Configuration (BGP, IS-IS, RIP), Router Configuration (BGP, IS-IS, OSPF, RIP)

[Contents] [Prev] [Next] [Index] [Report an Error]