[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls rsvp signalling hello graceful-restart recovery-time

#### Syntax

{ ip | mpls } rsvp signalling hello graceful-restart recovery-time recoveryTime

no { ip | mpls } rsvp signalling hello graceful-restart recovery-time

#### Release Information

Command introduced in JUNOSe Release 8.0.0.

#### Description

Configures the recovery time for RSVP-TE graceful restart for all interfaces that have RSVP-TE enabled. The no version restores the default value.

#### Options

- ip—Specifies alternative keyword for compatibility with non–E-series implementations
- recoveryTime—Time in milliseconds within which you want the neighboring routers to resynchronize RSVP-TE state and MPLS forwarding state after a graceful restart, in the range 60000–480000; default value is 120000

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]