[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

Symbols A B C D E F G H I J L M N O P Q R S T U V W X

Symbols

> 10-Gbps SRP module 1
> 10/100Base-T port 1
> –48 VDC 1

A

> access line modules 1
> access, management 1
>   setting up console 1
>   SNMP 1
>   Telnet setup 1
> accessing fan tray 1
> agency certification 1
> air filter 1
>   replacing 1
> airflow 1
>   rack-mounted installation and 1
>   specifications 1
> alarm ports 1
> amperage 1
> antistatic bags and containers 1
> assembly numbers, locating 1
> assigning an IP address 1

B

> BNC connector 1
> booting 1
>   LED activity 1

C

> cable-management bracket 1
>   installing 1
> cables 1
>   failure 1
>   I/O modules 1
>   pinouts 1
>   power input module 1
>   recommendations 1
>   redundant port 1
>   required 1
>   SRP I/O modules 1
> cabling 1
>   ERX routers 1
>   HSSI connectors 1
>   RJ-45 connectors 1
>   SC duplex connectors 1
>   SRP I/O modules 1
>   X.21/V.35 connectors 1
> Case Manager 1
> certifications 1
> circulation, air 1
> classification, packet 1
> cleaning 1
> CLI (command-line interface) 1
> clock source input ports 1
> clocking problems 1
> color code, power cable 1
> combinations of line modules 1
> command-line interface 1
> compliance 1
>   product reclamation and recycling 1
>   requirements 1
> components 1
>   returning 1
>   storing 1
> configuring cables 1
> configuring management access 1
> configuring Telnet 1
> connecting console to router 1
> connectors, pinouts 1
> console 1
>   for management access 1
>   ports 1
>     RS-232 1
> consumption, power 1
> conventions 1
>   notice icons 1
>   text and syntax 1
> current (electrical) requirements 1
> customer support 1
>   contacting JTAC 1

D

> DB-9 connector 1
> DC power 1
> detecting double-bit error 1
> Device Management System, NMC-RX 1
> diagnosing problems 1
> diagnostic LEDs 1
> dimensions of ERX routers 1
> dissipation, heat 1
> distribution rack 1
> documentation set 1
>   comments on 1
> double-bit errors 1
>   detecting 1
>   troubleshooting 1

E

> E-series routers 1
>   assigning IP address to 1
>   cabling 1
>   cabling recommendations 1
>   dimensions 1
>   electrical requirements 1
>   hardware 1
>   installing 1
>   installing components 1
>   installing modules 1
>   lifting 1
>   maintenance 1
>   management access 1
>   models 1
>   modules 1
>   power requirements 1
>   powering down 1
>   powering up 1
>   safety guidelines 1
>   site planning 1
>   slot groups and identification 1
>   space requirements 1
>   troubleshooting 1
> EIA distribution rack 1
> ejectors, module 1
> electrical requirements 1
> electronic equipment, recycling 1
> environmental requirements 1
> ERX-1440 router 1
> ERX-14xx models 1
>   fan tray 1
>   front view 1
>   rear view 1
> ERX-310 router 1
>   fan tray 1
>   front view 1
>   power cord warnings 1
>   rear view (AC model) 1
>   rear view (DC model) 1
> ERX-705 router 1
> ERX-7xx models 1
>   fan tray 1
>   front view 1
>   rear view 1
>   slot identification and grouping 1
> ESD (electrostatic discharge) 1
> ESD grounding jack, chassis 1
> Ethernet link 1
> external timing ports 1

F

> failure, fan 1
> failures 1
> FAN FAIL LED 1
> FAN OK LED 1
> fan tray 1
>   hot-swapping 1
> fans 1
>   failure 1
>   installing 1
>   location 1
>   redundancy 1
>   removing 1
>   status 1
> far-end receive failure 1
> FERF (far end receive failure) 1
> filler panel 1
> filter, air 1
> Flash cards 1
> flow, air 1

G

> grounding jack, ESD 1

H

> halt command 1
> hardware 1
>   cable configuration 1
>   reclamation and recycling 1
>   redundancy features 1
>   repairing and replacing 1
> hazardous materials, reclamation and recycling 1
> heat dissipation 1
> high-availability mode 1
> hot-swapping 1
>   fan trays 1
>   modules 1
> HSSI connectors, cabling 1
> humidity requirements 1
> HyperTerminal 1

I

> I/O modules 1
>   cables 1
>   installing 1
>   installing redundancy 1
>   OC48 Frame APS 1
>   removing 1
>   SFPs 1
>   SRP 1
> installing ERX routers 1
>   site planning 1
> installing modules 1
>   I/O modules 1
>   line modules 1
>   order of installation 1
>   slot groups and module arrangements 1
>   SRP I/O modules 1
>   SRP modules 1
> installing NVS cards 1
> installing redundancy I/O modules 1
> installing redundancy midplane 1
> installing SFPs 1
> installing spare line modules 1
> IP address, assigning 1

J

> JTAC, contacting 1

L

> lead in equipment, reclamation and recycling 1
> LEDs 1
>   abnormal activity 1
>   fans 1
>   line modules 1
>   normal activity 1
>   redundancy status 1
>   SRP modules 1
> lifting router 1
> line modules 1
>   access 1
>   combinations 1
>   installing 1
>   installing spare 1
>   LEDs 1
>   OC48 1
>   performance rate 1
>   redundancy 1
>   removing 1
>   slot groups 1
>   uplink 1
> location, for ERX routers 1

M

> maintenance, system 1
> management access 1
>   setting up console 1
>   SNMP 1
>   Telnet setup 1
> Management Information Bases 1
> management port 1
>   10/100Base-T 1
> managing modules 1
> manuals 1
>   comments on 1
> mechanical requirements for distribution rack 1
> memory, upgrading 1
> MIBs (Management Information Bases) 1
> midplane 1
>   redundancy 1
> models 1
>   ERX router 1
> module reset button 1
> modules 1
>   failure 1
>   hot-swapping 1
>   installing 1
>     order of installation 1
>   managing 1
>   removing 1
>   repairing and replacing 1
>   replacing 1
>   self-testing 1
>   storing 1
>   types of 1
> monitoring LEDs 1
> monitoring temperature 1
> mounting kits 1
> mounting posts for rack 1

N

> network management 1
>   setting up console 1
>   SNMP 1
>   Telnet setup 1
> NMC-RX Device Management System 1
> notice icons 1
> NVS cards 1
>   installing 1
>   storing 1

O

> OC48 modules 1
> ONLINE LED 1
> order of module installation 1

P

> packaging, recycling 1
> packet classification 1
> packing instructions 1
> PCMCIA slot, SRP modules 1
> performance rate, line modules 1
> PIM 1
>   replacing 1
> pinouts, router cables and connectors 1
> planning site for installation 1
> plenum 1
> ports 1
>   alarm 1
>   external timing 1
>   management 1
>   redundancy 1
>   status LEDs 1
> power 1
>   cabling power input module 1
>   consumption 1
>     system 1
>   dissipation 1
>   failures 1
>   redundancy 1
>   source A 1
>   source B 1
>   specifications 1
> power cord warnings 1
> power input module 1
>   cabling 1
>   replacing 1
> power requirements 1
> power switches 1
> powering down router 1
> powering up router 1
> preinstallation responsibilities 1
> preparing site for installation 1
> primary SRP module 1
> problems 1
> product numbers, locating 1

Q

> QoS, packet classification for 1

R

> rack, distribution 1
> reclamation and recycling 1
> recycling Juniper Networks equipment 1
> redundancy 1
>   line module status 1
>   midplane 1
>   SRP modules 1
>   status 1
> redundancy features (hardware) 1
>   fans 1
>   line modules 1
>   ports 1
>   SRP modules 1
> redundancy midplane 1
>   installing 1
> REDUNDANT LED 1
> release mechanisms for SFPs 1
> removing components 1
> removing modules 1
> removing SFPs 1
> repacking components 1
> repairing hardware components 1
> replacing components 1
> replacing modules 1
> replacing NVS cards 1
> replacing SFPs 1
> reset button, module 1
> Restriction of Hazardous Substances (RoHS) Directive, recycling equipment 1
> Return Materials Authorization 1
> returning product 1
> RJ-45 connectors, cabling 1
> RMA 1
> RoHS (Restriction of Hazardous Substances) Directive, recycling equipment 1
> RS-232 port 1

S

> safety 1
>   agency certification 1
>   guidelines 1
> SC duplex connectors, cabling 1
> self-testing, modules 1
> serial numbers, locating 1
> SFPs (small form-factor pluggable transceivers) 1
>   installing 1
>   removing 1
>   storing 1
> show configuration command 1
> show environment command 1
> show hardware command 1
> show version command 1
> show interface gigabitEthernet command 1
> site planning 1
> size 1
>   of ERX routers 1
>   of rack 1
> slot disable command 1
> slot groups 1
>   ERX-1410 router 1
>   ERX-7xx models 1
>   overloading 1
> small form-factor pluggable transceivers 1
> SMB connectors 1
> SNMP for management access 1
> SODIMMs 1
> software 1
>   configuration 1
>   upgrading 1
> space requirements 1
> spare line modules, installing 1
> specifications 1
>   airflow 1
>   dimensions 1
>   distribution rack 1
>   electrical 1
>   heat dissipation 1
>   space 1
>   weight 1
> SRP I/O modules 1
>   cabling 1
>   installing 1
>   removing 1
> SRP modules 1
>   errors on 1
>   installing 1
>   LEDs on 1
>   models 1
>   PCMCIA slot 1
>   powering down 1
>   redundancy 1
>   removing 1
> standby SRP module 1
> starting ERX routers 1
> status, redundancy 1
> storing, modules and components 1
> support, technical 1, See technical support
> switches, power 1
> switching on router 1
> switchover to spare line module 1
> synchronize command 1
> system maintenance 1

T

> technical support 1
>   contacting JTAC 1
> Telnet connection to router 1
> temperature 1
>   excessive 1
>   monitoring 1
>   requirements 1
> text and syntax conventions 1
> thermal protection mode 1
> timing inputs, external 1
> tools needed 1
> troubleshooting 1
>   booting 1
>   cables 1
>   clocking 1
>   double-bit errors 1
>   Ethernet link 1
>   fans 1
>   FERF 1
>   LED activity for 1
>   modules 1
>   power failure 1
>   safety guidelines 1

U

> uninstalling modules 1
> upgrading software 1
> uplink line modules 1

V

> ventilation 1
> voltage requirements 1

W

> warnings, safety 1
> Waste Electrical and Electronic Equipment (WEEE) Directive. 1, See WEEE Directive
> WEEE (Waste Electrical and Electronic Equipment) Directive, recycling equipment 1
> weight 1
>   of ERX routers 1
>   of rack 1
> wrist strap, antistatic 1

X

> X.21/V.35 connectors, cabling 1

[Contents] [Prev] [Next] [Index] [Report an Error]