[Contents] [Prev] [Next] [Index] [Report an Error]

# client-name

#### Syntax

client-name clientname

no client-name

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

From Domain Map Tunnel Configuration or Tunnel Group Tunnel Configuration mode, sets a hostname for a tunnel that the LAC uses when communicating with the LNS about the tunnel. The no version removes the hostname from the tunnel.

| Note: In Domain Map Tunnel Configuration mode, this command is replacing the hostname command. The hostname command may be removed completely from Domain Map Tunnel Configuration mode in a future release.

#### Options

- clientname—String of up to 64 characters (no spaces)

#### Mode

Domain Map Tunnel Configuration, Tunnel Group Tunnel Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]