[Contents] [Prev] [Next] [Index] [Report an Error]

# monitor atm vp

#### Syntax

monitor atm vp atm interfaceSpecifier vpi [ atm interfaceSpecifier vpi ]*
[ load-interval seconds ] [ display-time-of-day ]

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Displays bit rate and packet rate statistics over a specified time interval for one or more ATM virtual paths (VPs). There is no no version.

#### Options

- interfaceSpecifier—ATM interface specifier; see Interface Types and Specifiers
- vpi—Virtual path identifier of the PVC. The numeric range of the VPI depends on the line module capabilities and current configuration.
- seconds—Number of seconds in the range 5–300 that specifies the time interval at which the router calculates bit rates and packet rates for the specified VP; default value is 5 seconds
- display-time-of-day—Sets time at which the router calculates the bit rate and packet rate statistics for the current interval
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]