[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the COPS Layer Over SRC Connection

#### Purpose

Display information about the COPS layer over which the SRC connection is made.

#### Action

To display information about the COPS layer over which the SRC connection is made:

    host1#show cops info
    General Cops Information:

            Sessions Created: 1
            Sessions Deleted: 0
            Current Sessions: 1
            Bytes Received: 680
            Packets Received: 17
            Bytes Sent: 692
            Packets Sent: 21
            Keep Alive Received: 12
            Keep Alive Sent: 12

    Session Information
            Remote Ip Address: 10.10.0.223
            Remote TCP Port: 4001
            Client Type: 16384
            Bytes Received:   2224
            Packets Received: 5
            Bytes Sent:       596
            Packets Sent:     9
            REQ Sent:         4
            DEC Rcv:          4
            RPT Sent:         4
            DRQ Sent:         0
            SSQ Rcv:          0
            OPN Sent:         1
            CAT Rcv:          1
            CC Sent:          0
            CC Rcv:           0
            SSC Sent:         0

#### Meaning

Table 21 lists the show cops info command output fields.

Table 21: show cops info Output Fields

Field Name | Field Description
--- | ---
Session Created | Number of COPS sessions created
Sessions Deleted | Number of COPS sessions deleted
Current Sessions | Number of current COPS sessions
Bytes Received | Number of bytes received on all COPS sessions
Packets Received | Number of packets received on all COPS sessions
Bytes Sent | Number of bytes transmitted on all COPS sessions
Packets Sent | Number of packets transmitted on all COPS sessions
Keep Alive Received | Number of COPS keepalive messages received
Keep Alive Sent | Number of COPS keepalive messages sent
Remote IP Address | IP address of the remote pee
Remote TCP Port | TCP port number of the remote peer
Client Type | Type of client for the session. For this release the client type must be 16640 (SRC client).
Bytes Received | Number of bytes received for this COPS session
Packets Received | Number of packets received for this COPS session
Bytes Sent | Number of bytes sent on this COPS session
Packets Sent | Number of packets sent on this COPS session
REQ Sent | Number of Request packets sent on this COPS session
DEC Rcv | Number of Decision packets received on this COPS session
RPT Sent | Number of Report packets sent on this COPS session
DRQ Sent | Number of Delete Requests sent on this COPS session
SSQ Rcv | Number of Synch Requests received on this COPS session
OPN Sent | Number of Open messages sent on this COPS session
CAT Rcv | Number of Client Accepts packets received on this COPS session
CC Sent | Number of Client Closes packets sent on this COPS session
CC Rcv | Number of Client Closes packets received on this COPS session
SSC Sent | Number of Sync Complete packets sent on this COPS session

#### Related Topics

- show cops info

[Contents] [Prev] [Next] [Index] [Report an Error]