[Contents] [Prev] [Next] [Index] [Report an Error]

# atm bulk-config shutdown

#### Syntax

[ no ] atm bulk-config bulkConfigName shutdown
[ vc-range vpiStart vpiEnd vciStart vciEnd ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Administratively disables (shuts down) the specified VC range or subrange. The no version reenables the specified VC range or the specified subranges; this is the default condition.

#### Options

- bulkConfigName—Name of the VC range; string of up to 80 characters
- vpiStart—Starting virtual path identifier (inclusive) of the VC subrange you are configuring
- vpiEnd—Ending virtual path identifier (inclusive) of the VC subrange you are configuring
- vciStart—Starting virtual circuit identifier (inclusive) of the VC subrange you are configuring
- vciEnd—Ending virtual circuit identifier (inclusive) of the VC subrange you are configuring

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]