[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the Configuration of QoS Interface Sets

#### Purpose

Display information about configured interface sets.

#### Action

To display information about a specific interface set:

    host1#show qos-interface-set vlan-set
    interface                  member member restricted
       set    parent   port     type  count  interface
    --------- ------ --------- ------ ------ ----------
    vlan-set  vlan-ss lag test1 vlan   2        none

To display detailed information about a specific interface set:

    host1#show qos-interface-set vlan-set detail
    interface                   member member restricted
       set    parent    port     type  count  interface
    --------- ------- --------- ------ ------ ----------
    vlan-set  vlan-ss lag test1  vlan    2      none

    Children:
      vlan lag test1.1      vlan lag test1.4

#### Meaning

Table 53 lists the show qos-interface-set command output fields.

Table 53: show qos-interface-set Output Fields

Field Name | Field Description
--- | ---
interface set | Name of the interface set
parent | Name of the interface superset that is the parent of the interface set
port | Interface that is the parent of the interface superset
member type | Member-interface type defined for the interface set: vlan ip vlan
restricted interface | Restricted interface configured for this interface set
Children | List of interface members associated with the interface superset

#### Related Topics

- Configuring Interface Sets for QoS
- show qos-interface-set

[Contents] [Prev] [Next] [Index] [Report an Error]