[Contents] [Prev] [Next] [Index] [Report an Error]

# subscriber

#### Syntax

subscriber { bridgedEthernet | ip } { user | user-prefix } userName
domain domainName [ { password | password-prefix } password ]
[ no-authenticate ]

no subscriber { bridgedEthernet | ip }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures a local subscriber (when one cannot be obtained externally, as in PPP) on the E-series router to support authentication and configuration from the RADIUS server. The no version negates the command.

#### Options

- bridgedEthernet—Specifies bridgedEthernet as the upper interface type
- ip—Specifies IP as the upper interface type
- user—Employs the username as specified
- user-prefix—Appends the interface physical location to the username
- userName—RADIUS username
- domainName—Domain name
- password—Employs the password as specified
- password-prefix—Appends the interface physical location to the password
- password—RADIUS password
- no-authenticate—Disables authentication

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]