[Contents] [Prev] [Next] [Index] [Report an Error]

# slot ignore-diagnostic-failure

#### Syntax

[ no ] slot ignore-diagnostic-failure slotNum

#### Release Information

Command introduced in JUNOSe Release 9.3.0.

#### Description

Enables you to ignore diagnostics test failures on the line module or SRP. The no version returns you to the default allowing diagnostic test failures to occur.

#### Options

- slotNum—Number of the selected slot in the router; for ERX-7xx models, a number in the range 0–6; for ERX-14xx models, a number in the range 0–13; for the ERX-310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]