[Contents] [Prev] [Next] [Index] [Report an Error]

# excess-burst

#### Syntax

excess-burst { size | millisecond milliseconds }

no excess-burst

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets amount of bandwidth allocated to accommodate a packet in progress when the rate is in excess of the burst. The no version restores the default value, 0.

#### Options

- size—Amount of bandwidth allocated; in the range 0–4294967295
- milliseconds—Milliseconds in the range 1–10000

#### Mode

Rate Limit Profile Configuration

#### Related Topics

- Creating a Two-Rate Rate-Limit Profile

[Contents] [Prev] [Next] [Index] [Report an Error]