[Contents] [Prev] [Next] [Index] [Report an Error]

# radius connect-info-format

#### Syntax

radius connect-info-format { l2tp-connect-speed |
l2tp-connect-speed-rx-when-equal }

no radius connect-info-format

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the format of RADIUS attribute 77, Connect-Info, on the LNS. The format uses the received L2TP connect-speed AVPs that the LAC sends to the LNS. The no version restores the default, in which the LNS does not generate the Connect-Info attribute.

#### Options

- l2tp-connect-speed—Specifies that the Connect-Info attribute include only the RX speed when the RX speed is different from the TX speed and is greater than zero.
- l2tp-connect-speed-rx-when-equal—Specifies that the Connect-Info attribute always include the RX speed when the speed is greater than zero.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]