> - Download PDFs
> - retransmit

> # retransmit

> #### Syntax

> retransmit retries

> no retransmit

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Specifies maximum number of times the router retransmits a RADIUS packet to an authentication or accounting server. The no version restores the default value.

> #### Options

> - retries—Number of retries, in the range 0–16; default value is 3

> #### Mode

> RADIUS Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.