[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp dial-out max-buffered-triggers

#### Syntax

[ no ] l2tp dial-out max-buffered-triggers maxBuffers

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the maximum number of buffered trigger packets held for any dial-out session pending the successful establishment of the L2TP session. The no version set the number of trigger buffers to the default value, 0.

#### Options

- maxBuffers—Range 0–50 buffered packets

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]