[Contents] [Prev] [Next] [Index] [Report an Error]

# send-more-specific-routes-disable

#### Syntax

[ no ] send-more-specific-routes-disable

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that RIP does not send a more-specific route if it has a less-specific route with any metric. The no version restores the default condition, wherein RIP always sends a more-specific route even if a less-specific route with a metric is available.

#### Mode

Address Family Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]