[Contents] [Prev] [Next] [Index] [Report an Error]

# bridge snmp-trap link-status

#### Syntax

[ no ] bridge { bridgeGroupName | vplsName } snmp-trap link-status

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
vplsName variable added in JUNOSe Release 7.1.0.

#### Description

Enables SNMP link-status processing for all network interfaces associated with a bridge group or VPLS instance. The no version disables SNMP link-status processing for all interfaces in the bridge group or VPLS instance.

#### Options

- bridgeGroupName—Name of a bridge group specified with the bridge command
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command

#### Mode

Global Configuration

#### Related Topics

- Configuring Optional Attributes for VPLS Instances in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]