[Contents] [Prev] [Next] [Index] [Report an Error]

# ip use-framed-routes ip-subscriber

#### Syntax

[ no ] ip use-framed-routes ip-subscriber

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Configures the router to enable a static primary IP interface to use the RADIUS Framed-Route attribute [22]. The primary IP interface applies the framed routes as source IP addresses when creating and configuring dynamic subscriber interfaces. The no version disables the primary IP interface support of the Framed-Route RADIUS attribute.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]