[Contents] [Prev] [Next] [Index] [Report an Error]

# snmp-server interfaces rfc1213

#### Syntax

snmp-server interfaces rfc1213 [ maxIfIndex ] [ maxIfNumber ]

[ no ] snmp-server interfaces rfc1213

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that the router bases numbering in the IfTable on RFC 1213. The no version restores the default value, which is to use RFC 1573 style numbering in interface tables.

| Caution: Reducing the value of the maxIfIndex, the maxIfNumber, or both, causes the router to automatically reboot to factory default settings.

The router does not reboot to factory defaults if you:

#### Options

- Increase the values of maxIfIndex and/or maxIfNumber.
- Issue a no version of the snmp-server interfaces rfc1213 command when the router is already set up for RFC 1573 style numbering.
- Enter the snmp-server interfaces rfc1213 command with the same options multiple times.
- maxIfIndex—Maximum value of index numbers in the interface tables, in the range 100–65535; default value is 65535
- maxIfNumber—Maximum number of interfaces in each interface table, in the range 100–65535; default value is 65535

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]