[Contents] [Prev] [Next] [Index] [Report an Error]

# aps revert

#### Syntax

aps revert minutes

no aps revert

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the APS/MSP group to operate in revertive mode. The no version restores the default setting, nonrevertive mode.

#### Options

- minutes—Number of minutes in the range 5–12 at which the interface resumes the active role after that interface becomes available

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]