> - Download PDFs
> - vlan id
> - Related Topics
> - Configuring Ethernet/VLAN Layer 2 Services, Configuring Local ATM Cross-Connect with AAL5 Encapsulation, and Configuring Local Cross-Connects Between Ethernet/VLAN Interfaces in the JUNOSe BGP and MPLS Configuration Guide

> # vlan id

> #### Syntax

> vlan id idValue [ untagged ] [ mac-address macAddress ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Specifies a VLAN ID. There is no no version.

> #### Options

> - idValue—Number unique within the Ethernet interface, in the range 0–4095
> - untagged—Specifies that frames be sent untagged; valid only for VLAN ID 0
> - macAddress—MAC address of the interface; when you do not specify a unique MAC address, the VLAN uses the MAC address of the Ethernet interface

> #### Mode

> Interface Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.