[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp disable calling-number-avp

#### Syntax

[ no ] l2tp disable calling-number-avp

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Prevents the E-series LAC from sending the Calling Number attribute value pair (AVP) in incoming-call-request (ICRQ) packets. The no version enables sending of the Calling Number AVP, the default setting.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]